{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["自动测试项总表","人工测试项总表","自动测试记录表","常温检查测试表","自动测试记录表2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"自动测试项总表","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[[6,0,6,3]]}
["设备配置表"]
["设备名称","设备类型","设备型号","控制句柄"]
["频谱仪","频谱仪","E4440A","GPIB0::29::INSTR"]
["功率计","功率计","E4417A","GPIB0::21::INSTR"]
[]
["测试指标配置表"]
["通用配置项",null,null,null,"通道1"]
["测试指标","默认勾选","测试模板","测试顺序","测试参数配置表","启用状态"]
["常温检查","是","常温检查测试","1","常温检查测试表","启用"]

{"sheet":"人工测试项总表","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["人工测试项总表"]
["测试内容","技术要求","测试值/结果","测试结论"]
["功耗测试","<10W"]
["温度老练","老练后加电正常"]
["工作温度","<65℃"]

{"sheet":"自动测试记录表","index":2,"n_rows":12,"n_cols":13,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["通道","产品编号","相对时间\n(min)","绝对时间\n（MHz）","供电电压\n(V)","消耗电流\n(A)","输出频率\n(MHz)","调制频偏\n(dB)","调制频偏\n(KHz)","输出功率\n(W)","杂波抑制\n(dB)","谐波抑制\n（dB）","寄生调幅\n(%)"]
["CH1",null,0]
["CH1",null,5]
["CH1",null,10]
["CH1",null,20]
["CH1",null,30]
["CH2",null,0]
["CH2",null,5]
["CH2",null,10]
["CH2",null,20]
["CH2",null,30]

{"sheet":"常温检查测试表","index":3,"n_rows":59,"n_cols":5,"rows_kept":59,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["通道数","int","2"]
["起始频率","double","2100","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","1","产品测试的频点数量"]
["终止频率","double","2500","单位：MHz，产品的工作频带上限"]
["相位噪声偏置频率","double[]","0.1,1,10,100,1000","单位：KHz"]
["主频左侧偏移量","double","100","单位：MHz"]
["主频左侧起始值","double","1000","单位：MHz"]
["主频右侧偏移量","double","100","单位：MHz"]
["主频右侧终止值","double","3000","单位：MHz"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["小信号参考电平（REF）","string","-40","单位：dBm"]
["谐波次数","int[]","2,3,4,5","举例：测2次谐波，值为2，测2、3次谐波，值为2,3"]
["控制延时","int","5","单位：ms"]
["相对时间","int","1","单位：min"]
["测试次数","int","5"]
["电压下限","double","26","单位：V"]
["电压上限","double","29","单位：V"]
["电流下限","double","0.6","单位：A"]
["电流上限","double","1.2","单位：A"]
["功率下限","double","3.5","单位：W"]
["功率上限","double","20","单位：W"]
["最大频偏(KHz)下限","double","240","单位：KHz"]
["最大频偏(KHz)上限","double","320","单位：KHz"]
["杂波抑制下限","double","42","单位：dBc"]
["谐波抑制下限","double","45","单位：dBc"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["2GHz","-107±5",null,"-112","-102"]
["2.5GHz","-97±5",null,"-102","-92"]
[]
[]
[]
[]
[]
["串口","string","COM3"]
["起始频率","double","2100","单位：MHz,产品测试的起始频率"]
["频率步进","double","200","单位：MHz,产品测试的频率步进"]
["频点数量","int","10","产品测试的频点数量"]
["终止频率","double","2500","单位：MHz，产品的工作频带上限"]
["相位噪声偏置频率","double[]","0.1,1,10,100,1000","单位：KHz"]
["主频左侧偏移量","double","100","单位：MHz"]
["主频左侧起始值","double","1000","单位：MHz"]
["主频右侧偏移量","double","100","单位：MHz"]
["主频右侧终止值","double","3000","单位：MHz"]
["扫描带宽（SPAN）","string",250,"单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","3","单位：KHz"]
["视频带宽（VBW）","string","10","单位：KHz"]
["谐波次数","int[]","2,3,4,5","举例：测2次谐波，值为2，测2、3次谐波，值为2,3"]
["控制延时","int","5","单位：ms"]

{"sheet":"自动测试记录表2","index":4,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["测试内容","技术要求","上限值","下限值","IF1","IF2","IF3","IF4"]
["dBc/Hz@100Hz","<-92","-92","-100"]
["dBc/Hz@1KHz","<-93","-92","-100"]
["dBc/Hz@10KHz","<-94","-92","-100"]
["-3dB带宽",">13","20","13"]
["-40dB带宽",">25","30","25"]