{"text_format":"2","workbook":"xlsx","n_sheets":8,"sheets":["自动测试项总表","人工测试项总表","自动测试记录表","通道1增益测试表","通道1时钟相噪测试表","通道1带宽测试表","通道1镜频测试表","通道1相噪测试表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"自动测试项总表","index":0,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[[12,0,12,3]]}
["设备配置表"]
["设备名称","设备类型","设备型号","控制句柄"]
["信号源1","信号源","E4221B","GPIB0::10::INSTR"]
["信号源2","信号源","E4221B","GPIB0::11::INSTR"]
["频谱仪","频谱仪","E4440A","GPIB0::20::INSTR"]
["矢网","矢网","E5062A","GPIB0::21::INSTR"]
["示波器1","示波器","DSO-X 3024A","GPIB0::22::INSTR"]
["噪声系数分析仪1","噪声系数分析仪","N8975A","GPIB0::23::INSTR"]
["电子负载1","电子负载","IT8811","GPIB0::24::INSTR"]
["程控电源1","程控电源","IT6722","GPIB0::24::INSTR"]
[]
["测试指标配置表"]
["通用配置项",null,null,null,"通道1",null,"通道2",null,"通道3"]
["测试指标","默认勾选","测试模板","测试顺序","测试参数配置表","启用状态","测试参数配置表","启用状态","测试参数配置表","启用状态"]
["通道增益","是","增益测试模板","1","通道1增益测试表","启用","通道1增益测试表","启用","通道1增益测试表","启用"]
["相位噪声","否","相噪测试模板","2","通道1相噪测试表","启用","通道1相噪测试表","启用","通道1相噪测试表","启用"]
["镜频抑制","是","镜频测试模板","3","通道1镜频测试表","启用","通道1镜频测试表","启用","通道1镜频测试表","启用"]
["-3dB带宽","是","带宽测试模板","4","通道1带宽测试表","启用","通道1带宽测试表","启用","通道1带宽测试表","启用"]
["时钟相噪","是","时钟相噪测试模板","5","通道1时钟相噪测试表","启用","通道1时钟相噪测试表","启用","通道1时钟相噪测试表","启用"]

{"sheet":"人工测试项总表","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["人工测试项总表"]
["测试内容","技术要求","测试值/结果","测试结论"]
["功耗测试","<10W"]
["温度老练","老练后加电正常"]
["工作温度","<65℃"]

{"sheet":"自动测试记录表","index":2,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["测试内容","技术要求","上限值","下限值","IF1","IF2","IF3","IF4"]
["dBc/Hz@100Hz","<-92","-92","-100"]
["dBc/Hz@1KHz","<-93","-92","-100"]
["dBc/Hz@10KHz","<-94","-92","-100"]
["-3dB带宽",">13","20","13"]
["-40dB带宽",">25","30","25"]

{"sheet":"通道1增益测试表","index":3,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["频率","int[]","10,20,30","单位：MHz"]
["通道延迟","int",250,"单位：ms"]
[]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["2GHz","-107±5",null,"-112","-102"]
["2.5GHz","-97±5",null,"-102","-92"]

{"sheet":"通道1时钟相噪测试表","index":4,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["频率","int[]","11，22，33，44","单位：MHz",{"$nulls":4},"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["通道延迟","int",250,"单位：ms"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-92",null,"-92","-100"]
["dBc/Hz@1KHz","<-93",null,"-92","-100"]
["dBc/Hz@10KHz","<-94",null,"-92","-100"]

{"sheet":"通道1带宽测试表","index":5,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["频率","int[]","10,20,30","单位：MHz"]
["通道延迟","int",250,"单位：ms"]
[]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["-3dB带宽",">13",null,"20","13"]
["-40dB带宽",">25",null,"30","25"]

{"sheet":"通道1镜频测试表","index":6,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["频率","int[]","10,20,30","单位：MHz"]
["通道延迟","int",250,"单位：ms"]
[]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["镜像抑制","<-92",null,"-92","-100"]

{"sheet":"通道1相噪测试表","index":7,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["频率","int[]","11，22，33，44","单位：MHz"]
["通道延迟","int",250,"单位：ms"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-65",null,"-65","-70"]
["dBc/Hz@1KHz","<-75",null,"-75","-80"]
["dBc/Hz@10KHz","<-85",null,"-85","-90"]