{"text_format":"2","workbook":"xlsx","n_sheets":13,"sheets":["自动测试项总表","人工测试项总表","自动测试记录表","公共设置","通道1功率(功率计)测试表","通道1功率及频率稳定度测试表","通道1杂波抑制测试表","通道1谐波抑制测试表","通道1噪声功率谱密度测试表","通道1相位噪声测试表","通道1调制指数及最大频偏指标测试表","通道1FSK调制指数及最大频偏指标测试表","通道1电压及电流测试表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"自动测试项总表","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[[6,0,6,3]]}
["设备配置表"]
["设备名称","设备类型","设备型号","控制句柄"]
["功率计","功率计","EPM-441A","GPIB0::13::INSTR"]
["频谱仪","频谱仪","N9030A","USB0::0x0957::0x0D0B::US49230327::INSTR"]
[]
["测试指标配置表"]
["通用配置项",null,null,null,"通道1",null,"通道2"]
["测试指标","默认勾选","测试模板","测试顺序","测试参数配置表","启用状态","测试参数配置表","启用状态"]
["电压及电流","是","电压及电流测试","1","通道1电压及电流测试表","启用","通道1电压及电流测试表","启用"]
["功率(功率计)","是","功率(功率计)测试","2","通道1功率(功率计)测试表","启用","通道1功率(功率计)测试表","启用"]
["功率及频率稳定度","是","功率及频率稳定度测试","3","通道1功率及频率稳定度测试表","启用","通道1功率及频率稳定度测试表","启用"]
["杂波抑制","是","杂波抑制测试","4","通道1杂波抑制测试表","启用","通道1杂波抑制测试表","启用"]
["谐波抑制","是","谐波抑制测试","5","通道1谐波抑制测试表","启用","通道1谐波抑制测试表","启用"]
["噪声功率谱密度","是","噪声功率谱密度测试","6","通道1噪声功率谱密度测试表","启用","通道1噪声功率谱密度测试表","启用"]
["相位噪声","是","相位噪声测试","7","通道1相位噪声测试表","启用","通道1相位噪声测试表","启用"]
["调制指数及最大频偏指标","是","调制指数及最大频偏指标测试","8","通道1调制指数及最大频偏指标测试表","启用","通道1调制指数及最大频偏指标测试表","启用"]
["FSK调制指数及最大频偏指标","是","FSK调制指数及最大频偏指标测试","9","通道1FSK调制指数及最大频偏指标测试表","启用","通道1FSK调制指数及最大频偏指标测试表","启用"]

{"sheet":"人工测试项总表","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["人工测试项总表"]
["测试内容","技术要求","测试值/结果","测试结论"]
["功耗测试","<10W"]
["温度老练","老练后加电正常"]
["工作温度","<65℃"]

{"sheet":"自动测试记录表","index":2,"n_rows":2,"n_cols":5,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["名称","下限","上限","测试值","通过"]

{"sheet":"公共设置","index":3,"n_rows":7,"n_cols":7,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["电压","double","27","V"]
["电流","double","2","A"]
["程控电源","string","ASRL18::INSTR"]
["N9030A","string","USB0::0x0957::0x0D0B::US49230327::INSTR","频谱仪"]
["频点数","int","2","设置的值需小于等于该路径下串口控制文件中的频点数"]

{"sheet":"通道1功率(功率计)测试表","index":4,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["控制延时","int","10000","单位：ms"]
["功率下限","double","3","单位：W"]
["功率上限","double","999","单位：W"]
["两路功率总和下限","double","6","单位：W"]
["两路功率总和上限","double","999","单位：W"]
["功率不平度上限","double","1","单位：dB"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1功率及频率稳定度测试表","index":5,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["输出损耗","double","39","单位：dB"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["通道扫描带宽（SPAN）","string","1","单位：MHz"]
["通道带宽","string","1000","单位：KHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["控制延时","int","10000","单位：ms"]
["功率下限","double","3","单位：W"]
["功率上限","double","999","单位：W"]
["频率稳定度上限","double","0.00005"]
["两路功率总和下限","double","6","单位：W"]
["两路功率总和上限","double","999","单位：W"]
["功率不平度上限","double","1","单位：dB"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1杂波抑制测试表","index":6,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",{"$nulls":4},"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["主频左侧终止偏移量","double","20","单位：MHz"]
["主频左侧起始偏移量","double","250","单位：MHz"]
["主频右侧起始偏移量","double","20","单位：MHz"]
["主频右侧终止偏移量","double","250","单位：MHz"]
["特殊频点","double","1","单位：MHz,设置为0时，则表示不需要进行特殊频点测试"]
["扫描带宽（SPAN）","string","500","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","3000000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["小信号参考电平（REF）","string","-30","单位：dBm"]
["控制延时","int","10000","单位：ms"]
["临界偏移","double","0.1","单位：dB，用于判断测试值临界时在上下限的基础上偏多少范围内补偿"]
["抖动补偿","double","0.2","单位：dB"]
["杂波抑制下限","double","50","单位：dB"]
["杂波抑制上限","double","999","单位：dB"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1谐波抑制测试表","index":7,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["扫描带宽（SPAN）","string","0.5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["小信号参考电平（REF）","string","-20","单位：dBm"]
["谐波次数","int[]","2,3,4,5","举例：测2次谐波，值为2，测2、3次谐波，值为2,3"]
["控制延时","int","10000","单位：ms"]
["临界偏移","double","0.1","单位：dB，用于判断测试值临界时在上下限的基础上偏多少范围内补偿"]
["抖动补偿","double","0.2","单位：dB"]
["谐波抑制下限","double","50","单位：dB"]
["谐波抑制上限","double","999","单位：dB"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1噪声功率谱密度测试表","index":8,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["通道扫描带宽（SPAN）","string",100,"单位：MHz"]
["通道带宽","string","10000","单位：KHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["控制延时","int","10000","单位：ms"]
["噪声功率谱密度下限","double","-999","单位：dBm/Hz"]
["噪声功率谱密度上限","double","-70","单位：dBm/Hz"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1相位噪声测试表","index":9,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["相位噪声偏置频率","double[]","1000,10000","单位：Hz"]
["扫描带宽（SPAN）","string","1","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["相位噪声模式参考电平（REF）","string","-30","单位：dBc/Hz"]
["分辨率带宽（RBW）","string","300","单位：Hz"]
["视频带宽（VBW）","string","1000","单位：Hz"]
["控制延时","int","10000","单位：ms"]
["相位噪声下限","double","-999","单位：dBc"]
["相位噪声上限","double","-70","单位：dBc"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1调制指数及最大频偏指标测试表","index":10,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["控制延时","int","10000","单位：ms"]
["临界偏移","double","0.1","单位：dB，用于判断测试值临界时在上下限的基础上偏多少范围内补偿"]
["抖动补偿","double","0.2","调制系数补偿"]
["调制系数下限","double","0.6"]
["调制系数上限","double","0.8"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1FSK调制指数及最大频偏指标测试表","index":11,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",null,null,"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100000","单位：Hz"]
["视频带宽（VBW）","string","2000","单位：Hz"]
["控制延时","int","10000","单位：ms"]
["调制系数下限","double","0.6"]
["调制系数上限","double","0.8"]
["码率","double","5","Mbps"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]

{"sheet":"通道1电压及电流测试表","index":12,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["控制延时","int","10000","单位：ms"]
["电压下限","double","24","单位：V"]
["电压上限","double","31","单位：V"]
["电流下限","double","0.1","单位：A"]
["电流上限","double","1.5","单位：A"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]