{"text_format":"2","workbook":"xlsx","n_sheets":13,"sheets":["自动测试项总表","人工测试项总表","自动测试记录表4","自动测试记录表","自动测试记录表2","自动测试记录表1","通道1功率及频率稳定度测试表","通道1杂波抑制测试表","通道1谐波抑制测试表","通道1噪声功率谱密度测试表","通道1相位噪声测试表","通道1调制指数及最大频偏指标测试表","通道1电压及电流测试表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"自动测试项总表","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[6,0,6,3]]}
["设备配置表"]
["设备名称","设备类型","设备型号","控制句柄"]
["频谱仪","频谱仪","E4440A","GPIB0::29::INSTR"]
["功率计","功率计","E4417A","GPIB0::21::INSTR"]
[]
["测试指标配置表"]
["通用配置项",null,null,null,"通道1",null,"通道2"]
["测试指标","默认勾选","测试模板","测试顺序","测试参数配置表","启用状态","测试参数配置表","启用状态"]
["功率及频率稳定度","是","功率及频率稳定度测试","1","通道1功率及频率稳定度测试表","启用","通道1功率及频率稳定度测试表","启用"]
["杂波抑制","是","杂波抑制测试","2","通道1杂波抑制测试表","启用","通道1杂波抑制测试表","启用"]
["谐波抑制","是","谐波抑制测试","3","通道1谐波抑制测试表","启用","通道1谐波抑制测试表","启用"]
["噪声功率谱密度","是","噪声功率谱密度测试","4","通道1噪声功率谱密度测试表","启用","通道1噪声功率谱密度测试表","启用"]
["相位噪声","是","相位噪声测试","5","通道1相位噪声测试表","启用","通道1相位噪声测试表","启用"]
["调制指数及最大频偏指标","是","调制指数及最大频偏指标测试","6","通道1调制指数及最大频偏指标测试表","启用","通道1调制指数及最大频偏指标测试表","启用"]
["电压及电流","是","电压及电流测试","7","通道1电压及电流测试表","启用","通道1电压及电流测试表","启用"]

{"sheet":"人工测试项总表","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["人工测试项总表"]
["测试内容","技术要求","测试值/结果","测试结论"]
["功耗测试","<10W"]
["温度老练","老练后加电正常"]
["工作温度","<65℃"]

{"sheet":"自动测试记录表4","index":2,"n_rows":9,"n_cols":9,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["数据表","位置","通道号","测试项","名称","下限","上限","测试值","通过"]
["自动测试记录表1","E7：E21",null,null,"1AH-供电电压",null,null,5]
["自动测试记录表1","F7"]
[]
[]
[]
[{"$nulls":4},"1AH-消耗电流",null,null,8]
[{"$nulls":4},"2AH-消耗电流"]

{"sheet":"自动测试记录表","index":3,"n_rows":32,"n_cols":16,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["通道","产品编号","频率代码\nPL","设定频率\n（MHz）","发射机状态","供电电压\n（V）","消耗电流\n（A）","实际频率\n(MHz)","fL \n(MHz)","调制指数","输出功率(W)XY1E","输出功率(W)XY1F","两路功率总和\n(W)","功率不平度\n(dB)","杂波抑制\n（dB）","谐波抑制\n(dB)"]
["CH1",null,"1AH",2208.5,"开启"]
["CH1",null,"2AH",2214.5,"开启"]
["CH1",null,"3AH",2220.5,"开启"]
["CH1",null,"4AH",2226.5,"开启"]
["CH1",null,"5AH",2232.5,"开启"]
["CH1",null,"6AH",2238.5,"开启"]
["CH1",null,"7AH",2244.5,"开启"]
["CH1",null,"8AH",2250.5,"开启"]
["CH1",null,"9AH",2256.5,"开启"]
["CH1",null,"AAH",2262.5,"开启"]
["CH1",null,"BAH",2268.5,"开启"]
["CH1",null,"CAH",2274.5,"开启"]
["CH1",null,"DAH",2280.5,"开启"]
["CH1",null,"EAH",2286.5,"开启"]
["CH1",null,"FAH",2292.5,"开启"]
["CH2",null,"1AH",2208.5,"开启"]
["CH2",null,"2AH",2214.5,"开启"]
["CH2",null,"3AH",2220.5,"开启"]
["CH2",null,"4AH",2226.5,"开启"]
["CH2",null,"5AH",2232.5,"开启"]
["CH2",null,"6AH",2238.5,"开启"]
["CH2",null,"7AH",2244.5,"开启"]
["CH2",null,"8AH",2250.5,"开启"]
["CH2",null,"9AH",2256.5,"开启"]
["CH2",null,"AAH",2262.5,"开启"]
["CH2",null,"BAH",2268.5,"开启"]
["CH2",null,"CAH",2274.5,"开启"]
["CH2",null,"DAH",2280.5,"开启"]
["CH2",null,"EAH",2286.5,"开启"]
["CH2",null,"FAH",2292.5,"开启"]

{"sheet":"自动测试记录表2","index":4,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["自动测试记录表"]
["测试内容","技术要求","上限值","下限值","IF1","IF2","IF3","IF4"]
["dBc/Hz@100Hz","<-92","-92","-100"]
["dBc/Hz@1KHz","<-93","-92","-100"]
["dBc/Hz@10KHz","<-94","-92","-100"]
["-3dB带宽",">13","20","13"]
["-40dB带宽",">25","30","25"]

{"sheet":"自动测试记录表1","index":5,"n_rows":24,"n_cols":15,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,0,1,14],[2,1,2,14],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[23,0,23,14],[4,14,5,14],[6,0,20,0],[6,13,20,13],[6,14,20,14],[21,1,21,14],[22,1,22,14],[4,7,5,7],[4,8,5,8],[4,9,4,10],[4,11,5,11],[4,12,5,12],[4,13,5,13]]}
["自动测试记录表"]
["(发射机)"]
["测试项目","常温测试"]
["技术要求","依据技术条件中表3的频率代码，逐一在信号源中输入，命令帧格式见技术条件中表2所示，其中的PL为一个字节的频率代码，启动发送后，应在频谱仪上看到与相应的设置理论中心频率对应的频谱，记录实际的中心频率，若|实际频率-理论频率|÷理论频率≤5 X 10-5，则中心频率满足指标要求。调制指数：0.7±0.1；功率：两路总和≥6W,功率不平度不大于1dB；杂波抑制：不小于50dB；谐波抑制：不小于50dB。"]
["产品编号","频率代码\nPL","设定频率\n（MHz）","发射机状态","供电电压\n（V）","消耗电流\n（A）","实际频率\n(MHz)","fL\n(MHz)","调制指数","输出功率(W)",null,"两路功率总和\n(W)","功率不平度\n(dB)","杂波抑制\n（dB）","谐波抑制\n(dB)"]
[{"$nulls":9},"XY1E","XY1F"]
[null,"1AH",2208.5,"开启"]
[null,"2AH",2214.5,"开启"]
[null,"3AH",2220.5,"开启"]
[null,"4AH",2226.5,"开启"]
[null,"5AH",2232.5,"开启"]
[null,"6AH",2238.5,"开启"]
[null,"7AH",2244.5,"开启"]
[null,"8AH",2250.5,"开启"]
[null,"9AH",2256.5,"开启"]
[null,"AAH",2262.5,"开启"]
[null,"BAH",2268.5,"开启"]
[null,"CAH",2274.5,"开启"]
[null,"DAH",2280.5,"开启"]
[null,"EAH",2286.5,"开启"]
[null,"FAH",2292.5,"开启"]
["备注"]
["结论","本页检验    台合格，    台不合格。"]
["检验员：               测试日期：                 温度：                       湿度：              %"]

{"sheet":"通道1功率及频率稳定度测试表","index":6,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["控制延时","int","5","单位：ms"]
["功率下限","double","3.5","单位：W"]
["功率上限","double","20","单位：W"]
["频率稳定度上限","double","0.00005"]
["两路功率总和下限","double","6","单位：W"]
["功率不平度上限","double","1","单位：dB"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["2GHz","-107±5",null,"-112","-102"]
["2.5GHz","-97±5",null,"-102","-92"]

{"sheet":"通道1杂波抑制测试表","index":7,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注",{"$nulls":4},"byte,byte[],int,int[],uint,uint[],double,double[],string,string[],bool,bool[],short,short[],ushort,ushort[],Int64,Int64[],uint64,uint64[]"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["主频左侧偏移量","double","100","单位：MHz"]
["主频左侧起始值","double","1000","单位：MHz"]
["主频右侧偏移量","double","100","单位：MHz"]
["主频右侧终止值","double","3000","单位：MHz"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["小信号参考电平（REF）","string","-40","单位：dBm"]
["控制延时","int","5","单位：ms"]
["杂波抑制下限","double","50","单位：dBc"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-92",null,"-92","-100"]
["dBc/Hz@1KHz","<-93",null,"-92","-100"]
["dBc/Hz@10KHz","<-94",null,"-92","-100"]

{"sheet":"通道1谐波抑制测试表","index":8,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["小信号参考电平（REF）","string","-40","单位：dBm"]
["谐波次数","int[]","2,3,4,5","举例：测2次谐波，值为2，测2、3次谐波，值为2,3"]
["控制延时","int","5","单位：ms"]
["谐波抑制下限","double","50","单位：dBc"]
[]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["-3dB带宽",">13",null,"20","13"]
["-40dB带宽",">25",null,"30","25"]

{"sheet":"通道1噪声功率谱密度测试表","index":9,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["控制延时","int","5","单位：ms"]
["噪声功率谱密度上限","double","-70","单位：dBm/Hz"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["镜像抑制","<-92",null,"-92","-100"]

{"sheet":"通道1相位噪声测试表","index":10,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["相位噪声偏置频率","double[]","0.1,1,10,100,1000","单位：KHz"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["控制延时","int","5","单位：ms"]
["相位噪声上限","double","-70","单位：dBc"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-65",null,"-65","-70"]
["dBc/Hz@1KHz","<-75",null,"-75","-80"]
["dBc/Hz@10KHz","<-85",null,"-85","-90"]

{"sheet":"通道1调制指数及最大频偏指标测试表","index":11,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["输出损耗","double","30"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","100","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["控制延时","int","5","单位：ms"]
["调制系数下限","double","0.6"]
["调制系数上限","double","0.8",{"$nulls":4},"point"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-65",null,"-65","-70"]
["dBc/Hz@1KHz","<-75",null,"-75","-80"]
["dBc/Hz@10KHz","<-85",null,"-85","-90"]

{"sheet":"通道1电压及电流测试表","index":12,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["参数表"]
["名称","类型","值","备注"]
["串口","string","COM3"]
["起始频率","double","2208.5","单位：MHz,产品测试的起始频率"]
["频率步进","double","0","单位：MHz,产品测试的频率步进"]
["频点数量","int","15","产品测试的频点数量"]
["终止频率","double","2292.5","单位：MHz，产品的工作频带上限"]
["扫描带宽（SPAN）","string","5","单位：MHz"]
["参考电平（REF）","string","10","单位：dBm"]
["分辨率带宽（RBW）","string","10","单位：KHz"]
["视频带宽（VBW）","string","3","单位：KHz"]
["控制延时","int","5","单位：ms"]
["电压下限","double","26","单位：V"]
["电压上限","double","29","单位：V"]
["电流下限","double","0.6","单位：A"]
["电流上限","double","1.2","单位：A"]
[]
["测试显示表"]
["测试内容","技术要求","测试结果","上限值","下限值"]
["dBc/Hz@100Hz","<-65",null,"-65","-70"]
["dBc/Hz@1KHz","<-75",null,"-75","-80"]
["dBc/Hz@10KHz","<-85",null,"-85","-90"]