{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":95,"n_cols":5,"rows_kept":95,"cut":false,"hidden":false,"merged":[]}
["功率变化(dB)","调制指数(mf)","最大频偏(KHz)",null,"调制指数保留三位有效小数，频偏（仪器测试端）保留2位有效小数，最大频偏保留2有效小数"]
[13.8,0.4,163.84]
[13.69,0.40500000000000003,165.89]
[13.58,0.41000000000000003,167.94]
[13.47,0.41500000000000004,169.98]
[13.36,0.42000000000000004,172.03]
[13.25,0.42500000000000004,174.08]
[13.15,0.43000000000000005,176.13]
[13.04,0.43500000000000005,178.18]
[12.94,0.44,180.22]
[12.83,0.44500000000000001,182.27]
[12.73,0.45,184.32]
[12.63,0.45500000000000002,186.37]
[12.53,0.46,188.42]
[12.43,0.46500000000000002,190.46]
[12.33,0.47000000000000003,192.51]
[12.24,0.47500000000000003,194.56]
[12.14,0.48000000000000004,196.61]
[12.04,0.48500000000000004,198.66]
[11.95,0.49,200.7]
[11.86,0.495,202.75]
[11.76,0.5,204.8]
[11.67,0.505,206.85]
[11.58,0.51,208.9]
[11.49,0.51500000000000001,210.94]
[11.4,0.52,212.99]
[11.31,0.52500000000000002,215.04]
[11.22,0.53,217.09]
[11.13,0.53500000000000003,219.14]
[11.05,0.54,221.18]
[10.96,0.54500000000000004,223.23]
[10.87,0.55000000000000004,225.28]
[10.79,0.55500000000000005,227.33]
[10.7,0.56000000000000005,229.38]
[10.62,0.56500000000000006,231.42]
[10.54,0.57000000000000006,233.47]
[10.46,0.57500000000000007,235.52]
[10.37,0.58000000000000007,237.57]
[10.29,0.58499999999999996,239.62]
[10.210000000000001,0.59000000000000008,241.66]
[10.130000000000001,0.59499999999999997,243.71]
[10.050000000000001,0.60000000000000009,245.76]
[9.9700000000000006,0.60499999999999998,247.81]
[9.89,0.61,249.86]
[9.82,0.61499999999999999,251.9]
[9.74,0.62,253.95]
[9.66,0.625,256]
[9.58,0.63,258.05]
[9.51,0.63500000000000001,260.10000000000002]
[9.43,0.64,262.14]
[9.36,0.64500000000000002,264.19]
[9.2799999999999994,0.65,266.24]
[9.2100000000000009,0.65500000000000003,268.29000000000002]
[9.1300000000000008,0.66,270.33999999999997]
[9.06,0.66500000000000004,272.38]
[8.99,0.67,274.43]
[8.91,0.67500000000000004,276.48]
[8.84,0.68,278.52999999999997]
[8.77,0.68500000000000005,280.58]
[8.6999999999999993,0.69,282.62]
[8.6300000000000008,0.69500000000000006,284.67]
[8.56,0.7,286.72000000000003]
[8.49,0.70500000000000007,288.77]
[8.42,0.71,290.82]
[8.35,0.71500000000000008,292.86]
[8.2799999999999994,0.72,294.91000000000003]
[8.2100000000000009,0.72500000000000009,296.95999999999998]
[8.14,0.73,299.01]
[8.07,0.7350000000000001,301.06]
[8,0.74,303.10000000000002]
[7.94,0.74500000000000011,305.14999999999998]
[7.87,0.75,307.2]
[7.8,0.755,309.25]
[7.74,0.76,311.3]
[7.67,0.76500000000000001,313.33999999999997]
[7.6,0.77,315.39]
[7.54,0.77500000000000002,317.44]
[7.47,0.78,319.49]
[7.41,0.78500000000000003,321.54000000000002]
[7.34,0.79,323.58]
[7.28,0.79500000000000004,325.63]
[7.21,0.8,327.68]
[7.15,0.80500000000000005,329.73]
[7.09,0.81,331.78]
[7.02,0.81500000000000006,333.82]
[6.96,0.82000000000000006,335.87]
[6.9,0.82499999999999996,337.92]
[6.83,0.83000000000000007,339.97]
[6.77,0.83499999999999996,342.02]
[6.71,0.84000000000000008,344.06]
[6.64,0.84499999999999997,346.11]
[6.58,0.85000000000000009,348.16]
[6.52,0.85499999999999998,350.21]
[6.46,0.8600000000000001,352.26]
[6.4,0.86499999999999999,354.3]