{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["序号","串口号","第3个字节","第4个字节","频点(MHz)","字节是从左往右数"]
["1","COM17","02","01","2238.5"]
["2",null,null,"02","2268.5"]
["3",null,null,"03","2226.5"]
["4",null,null,"04","2286.5"]
["5",null,null,"05","2250.5"]
["6",null,null,"06","2280.5"]
["7",null,null,"07","2214.5"]
["8",null,null,"08","2244.5"]
["9",null,null,"09","2256.5"]
["10",null,null,"0A","2262.5"]
["11",null,null,"0B","2232.5"]
["12",null,null,"0C","2274.5"]
["13",null,null,"0D","2220.5"]
["14",null,null,"0E","2208.5"]
["15",null,null,"0F","2292.5"]