{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":5,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["功率变化(dB)","调制指数(mf)","最大频偏(KHz)",null,"调制指数保留三位有效小数，频偏（仪器测试端）保留2位有效小数，最大频偏保留2有效小数"]
[10.050000000000001,0.6,245.76]
[9.9700000000000006,0.60499999999999998,247.81]
[9.89,0.61,249.86]
[9.82,0.61499999999999999,251.9]
[9.74,0.62,253.95]
[9.66,0.625,256]
[9.58,0.63,258.05]
[9.51,0.63500000000000001,260.10000000000002]
[9.43,0.64,262.14]
[9.36,0.64500000000000002,264.19]
[9.2799999999999994,0.65,266.24]
[9.2100000000000009,0.65500000000000003,268.29000000000002]
[9.1300000000000008,0.65999999999999992,270.33999999999997]
[9.06,0.66500000000000004,272.38]
[8.99,0.66999999999999993,274.43]
[8.91,0.67499999999999993,276.48]
[8.84,0.67999999999999994,278.52999999999997]
[8.77,0.68499999999999994,280.58]
[8.6999999999999993,0.69,282.62]
[8.6300000000000008,0.69499999999999995,284.67]
[8.56,0.7,286.72000000000003]
[8.49,0.70499999999999996,288.77]
[8.42,0.71,290.82]
[8.35,0.71499999999999997,292.86]
[8.2799999999999994,0.72,294.91000000000003]
[8.2100000000000009,0.72499999999999998,296.95999999999998]
[8.14,0.73,299.01]
[8.07,0.73499999999999999,301.06]
[8,0.74,303.10000000000002]
[7.94,0.745,305.14999999999998]
[7.87,0.75,307.2]
[7.8,0.755,309.25]
[7.74,0.76,311.3]
[7.67,0.76500000000000001,313.33999999999997]
[7.6,0.77,315.39]
[7.54,0.77500000000000002,317.44]
[7.47,0.78,319.49]
[7.41,0.78499999999999992,321.54000000000002]
[7.34,0.79,323.58]
[7.28,0.79499999999999993,325.63]
[7.21,0.8,327.68]
[7.15,0.80499999999999994,329.73]
[7.09,0.80999999999999994,331.78]
[7.02,0.81499999999999995,333.82]
[6.96,0.82,335.87]
[6.9,0.82499999999999996,337.92]
[6.83,0.83,339.97]
[6.77,0.83499999999999996,342.02]
[6.71,0.84,344.06]
[6.64,0.84499999999999997,346.11]
[6.58,0.85,348.16]